[**Ausschreibungstext**](http://www.ausschreiben.de/online/usr/show.php?tb=richter_kunststofftechnik&ade=0&showtree=1&ids=8&tbframe=richter_kunststofftechnik)

Biovitor DN 150 - Regenwasserfilter,

biologischer Absetzfilter DN 150, für Dachflächen bis 340 m², mit integriertem Zulaufberuhiger

Mögliche Anschlussgrößen: DN 160

Biovitor DN 150, Regenwasserfilter mit biologischem Wirkprinzip, inklusive Zulaufberuhiger, Wartung nur alle 10 Jahre bei vorgeschaltetem Laubabscheider, kein Höhenversatz zwischen Zu- und Ablauf in der Zisterne notwendig, Montage auf dem Zisternenboden, für alle Zisternen mit einer Einstiegsöffnung DN 600 nachrüstbar!

Anschließbare Dachflächen, Anschlusskapazität nach DIN 1986, bei einer Regenspende von:

max. 200 l/(s\*ha) 600 m²

max. 300 l/(s\*ha)  340 m²

Bei starkem Laubanfall sollte der Anlage ein grober Laubabscheider (Dachrinnengitter) vorgeschaltet werden!

Gewicht: 47 kg

Durchmesser: 550 mm

Höhe: 1.960 mm

Artikelnummer: G0002975

Mengeneinheit: Stück

Herstellerangaben:

GreenLife GmbH

Sacktannen 1a

19057 Schwerin

Telefon +49 (0) 385 – 77337-0

Telefax +49 (0) 385 – 77337-33

Web www.greenlife.info

E-Mail info@greenlife.info

Menge: ………… Einheit: **Stk**. EP: ………… GP: …………

[**tender**](http://www.ausschreiben.de/online/usr/show.php?tb=richter_kunststofftechnik&ade=0&showtree=1&ids=8&tbframe=richter_kunststofftechnik) **specifications**

Biovitor DN 150 – rainwater filter

Biological settling filter DN 150, for connectable roof surfaces of up to 340 m², with integrated calmed inlet

possible connection sizes: DN 160

Biovitor DN 150, rainwater filter with biological principle, including calmed inlet, maintenance only every 10 years with upstream gutter guards, no height offset between inflow and overflow in the tank necessary, can be installed on the tank bottom, can be retrofitted for all cisterns with a DN 600 entrance opening!  
Connectable roof surfaces, connection capacity according to DIN 1986, with a rain donation of:  
max. 200 l/(s\*ha) 600 m²  
max. 300 l/(s\*ha) 340 m²

If the leaf fall is strong, a coarse leave separator (gutter guard) should be installed upstream!

weight: 47 kg  
diameter: 550 mm  
height: 1.960 mm  
item no.: G0002975  
unit of quantity: piece

manufacturer:

GreenLife GmbH

Sacktannen 1a

D-19057 Schwerin

Germany

phone +49 (0) 385 – 77337-0

fax +49 (0) 385 – 77337-33

web www.greenlife.info

e-mail info@greenlife.info

quantity: ………… unit: **piece** single price: ………… total price: …………