**[Ausschreibungstext](http://www.ausschreiben.de/online/usr/show.php?tb=richter_kunststofftechnik&ade=0&showtree=1&ids=8&tbframe=richter_kunststofftechnik" \o "Ausschreibungstext einblenden bzw. ausblenden)**

Biovitor DN 300 - Regenwasserfilter,

biologischer Absetzfilter DN 300, für Dachflächen bis 2.200 m², mit integriertem Zulaufberuhiger

Mögliche Anschlussgrößen: DN 300

Biovitor DN 300, Regenwasserfilter mit biologischem Wirkprinzip, inklusive Zulaufberuhiger, Wartung nur alle 10 Jahre bei vorgeschaltetem Laubabscheider, kein Höhenversatz zwischen Zu- und Ablauf in der Zisterne notwendig, Montage auf dem Zisternenboden!

Anschließbare Dachflächen, Anschlusskapazität nach DIN 1986, bei einer Regenspende von:

max. 200 l/(s\*ha) 5.600 m²

max. 300 l/(s\*ha)  2.200 m²

Bei starkem Laubanfall sollte der Anlage ein grober Laubabscheider (Dachrinnengitter) vorgeschaltet werden!

Gewicht: 160 kg

Durchmesser: 1.250 mm

Höhe: 2.675 mm

Artikelnummer: G0002977

Mengeneinheit: Stück

Herstellerangaben:

GreenLife GmbH

Sacktannen 1a

19057 Schwerin

Telefon +49 (0) 385 – 77337-0

Telefax +49 (0) 385 – 77337-33

Web www.greenlife.info

E-Mail info@greenlife.info

Menge: ………… Einheit: **Stk**. EP: ………… GP: …………

[**tender**](http://www.ausschreiben.de/online/usr/show.php?tb=richter_kunststofftechnik&ade=0&showtree=1&ids=8&tbframe=richter_kunststofftechnik) **specifications**

Biovitor DN 300 – rainwater filter

Biological settling filter DN 300, for connectable roof surfaces of up to 2.200 m², with integrated calmed inlet

possible connection sizes: DN 300

Biovitor DN 300, rainwater filter with biological principle, including calmed inlet, maintenance only every 10 years with upstream gutter guards, no height offset between inflow and overflow in the tank necessary, can be installed on the tank bottom!  
Connectable roof surfaces, connection capacity according to DIN 1986, with a rain donation of:  
max. 200 l/(s\*ha) 5.600 m²  
max. 300 l/(s\*ha) 2.200 m²

If the leaf fall is strong, a coarse leave separator (gutter guard) should be installed upstream!

weight: 160 kg  
diameter: 1.250 mm  
height: 2.675 mm  
item no.: G0002977  
unit of quantity: piece

manufacturer:

GreenLife GmbH

Sacktannen 1a

D-19057 Schwerin

Germany

phone +49 (0) 385 – 77337-0

fax +49 (0) 385 – 77337-33

web www.greenlife.info

e-mail info@greenlife.info

quantity: ………… unit: **piece** single price: ………… total price: …………